M-File Help: mdl_puma560akb | View code for mdl_puma560akb

# mdl_puma560akb

Create model of Puma 560 manipulator

    mdl_puma560akb

Script creates the workspace variable p560m which describes the kinematic and dynamic characterstics of a Unimation Puma 560 manipulator modified DH conventions.

Also defines the workspace vectors:

qz | zero joint angle configuration
qr | vertical 'READY' configuration
qstretch | arm is stretched out in the X direction

## References

- "The Explicit Dynamic Model and Inertial Parameters of the Puma 560 Arm" Armstrong, Khatib and Burdick 1986

## See also

SerialLink, mdl_puma560, mdl_stanford, mdl_twolink

© 1990-2014 Peter Corke.